| Reading a potentiometer by BARRAGAN <http://barraganstudio.com> Reads values from a potentiometer connected to the analog input pin 0. The value read from the sensor is proportional to the knob position on the potentiomenter. The value read is printed through the serial to be monitored using the serial monitor. Created 4 April 2007 |

    // Reading a potentiometer
    // by BARRAGAN <http://barraganstudio.com>

    int val;

    void setup()
    {
      Serial.begin(9600);           // sets the serial port to 9600
    }

    void loop()
    {
      val = analogRead(0);          // read analog input pin 0
      Serial.print(val, DEC);       // prints the value read
      Serial.print(" ");            // prints a space betwen the numbers
      delay(100);                   // wait 100ms for next reading
    }