| Index

| Reference for Wiring 1.0 (ALPHA) 0020+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### pulseStop()
Examples |  |
    void setup() {
      pinMode(0, INPUT);  // sets digital pin 0 as input to connect a switch
      pulseOut(4, 20);  // generates a pulse of 20Hz on PWM output pin 4
    }

    void loop() {
      if(digitalRead(0) == HIGH) {  // if the switch is pressed stop the pulse
        pulseStop(4);
      }
    }
Description |  | The pulseStop() method stops the pulse generation in the specified PWM output pin. If a number of pulses has been specified it stops the pulses even if there is remaining pulses to generate.
Syntax |  |
    pulseStop(pin)
Parameters |  |
pin |  | int: the PWM output pin number to stop generating pulses
Returns |  | None
Usage |  | Application
Related |  | pulseOut() pulseRunning()