| Index

| Reference for Wiring 1.0 (ALPHA) 0021+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### read()
Examples |  |
    #include <QSlide.h>

    /* create a new QSlide instance
       pin 2: data ready   (drdy)
       pin 3: data in      (sdi)
       pin 4: slave select (ss)
       pin 5: clock        (sclk)
       pin 6: data out     (sdo)
       pin 7: detect       (detect)
       pin 8: proximity    (prox)
    */
    QSlide slider = QSlide(2, 3, 4, 5, 6, 7, 8);

    void setup()
    {
      Serial.begin(9600);      // begin serial communication at 9600bps
    }

    void loop()
    {
      if(slider.isTouching())  // if someone is touching the slider
      {
        int x = slider.read(); // read the slider as an integer
        Serial.print(x);       // print via serial port
      }
    }
Description |  | The read() method returns the value read from the QSlide sensor.
Syntax |  |
    slider.read()
Parameters |  |
slider |  | The QSlide object
Returns |  | int
Usage |  | Application