| International Rectifiers IRLD024 Mosfet Switch by BARRAGAN <http://barraganstudio.com> A Mosfet is s special kind of transistor switch used to handle higher loads than the Wiring board can handle by itself. Logic-level MOSFETs can be connected directly to a Wiring I/O board output pin. In this example the Wiring board is blinking a 12V lamp by using an IRLD024 Mosfet connected to the digital Pin 0 Don't forget to tie together the Wiring GND and the Lamp 12V power supply GND. Created 7 January 2007 |

    // International Rectifiers IRLD024 Mosfet Switch
    // by BARRAGAN <http://barraganstudio.com>

    int mosfetPin = 0;           // Mosfet Gate pin connected to the Wiring I/O board pin 0

    void setup()
    {
      pinMode(mosfetPin, OUTPUT); // sets the digital pin as output
    }

    void loop()
    {
      digitalWrite(mosfetPin, HIGH);   // sets the Lamp on
      delay(1000);                  // waits for a second
      digitalWrite(mosfetPin, LOW);    // sets the Lamp off
      delay(1000);
    }

|  | .