| Index

| Reference for Wiring 1.0 (ALPHA) 0022+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### << (Bitwise bit shift left)
Examples |  |
    unsigned int value=4;                //  4 = 0000 0100
    unsigned int shift=2;

    value = value << shift;        // 16 = 0001 0000
    value <<= shift;               // 64 = 0100 0000
Description |  | The left expressions value is moved left by the number of bits specified by the right expression.
Syntax |  |
    expression1 << expression2
    expression1 <<= expression2
Parameters |  |
expression1 |  | any valid expression
expression2 |  | any valid expression
Returns |  |
Usage |  | Application
Related |  | & (bitwise AND) &= (bitwise AND and assign) | (bitwise OR) |= (bitwise OR and assign) ^ (bitwise XOR) ˜ (bitwise ones complement) >> (bitwise bit shift right)