| Index

| Reference for Wiring 1.0 (ALPHA) 0022+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Class |  | Library
Name |  | ### write()
Examples |  |
    #include <Servo.h>

    Servo myservo;

    void setup() {
      myservo.attach(2)  // attaches a servo connected to pin 2
    }

    void loop() {
      myservo.write(90);  // sets the servo position at 90 degrees
    }
    #include <Servo.h>

    Servo myservo;

    void setup() {
      myservo.attach(3) // attaches a servo connected to pin 3
    }

    void loop() {
      myservo.write(180);  // sets the servo position at 180 degrees
    }
Description |  | The write(degrees) method sets the position of the servo to the degrees specified. Servos can be positioned between 0 and 180 degrees. An invalid angle that is valid as pulse in microseconds is treated as microseconds.
Syntax |  |
    servo.write(degrees)
Parameters |  |
servo |  | Any variable of type Servo
degrees |  | Any integer value between 0 and 180
Returns |  | None
Usage |  | Application