| Advanced Output by Nicholas Zambetti <http://www.zambetti.com> Demonstrates printing with the Serial library Uses a variety of print calls to output the ASCII character mapping Created 29 March 2006 |

    // Advanced Output
    // by Nicholas Zambetti <http://www.zambetti.com>

    void setup()
    {
      Serial.begin(9600);

      // prints title with ending line break
      Serial.println("ASCII Table ~ Character Map");

      // wait for the long string to be sent
      delay(100);
    }

    int number = 33; // first visible character '!' is #33

    void loop()
    {
      Serial.print(number, BYTE);    // prints value unaltered, first will be '!'

      Serial.print(", dec: ");
      Serial.print(number);          // prints value as string in decimal (base 10)
      // Serial.print(number, DEC);  // this also works

      Serial.print(", hex: ");
      Serial.print(number, HEX);     // prints value as string in hexadecimal (base 16)

      Serial.print(", oct: ");
      Serial.print(number, OCT);     // prints value as string in octal (base 8)

      Serial.print(", bin: ");
      Serial.println(number, BIN);   // prints value as string in binary (base 2)
                                     // also prints ending line break

      // if printed last visible character '~' #126 ...
      if(number == 126) {
        // loop forever
        while(true) {
          continue;
        }
      }

      number++; // to the next character

      delay(100); // allow some time for the Serial data to be sent
    }