Search wiring.org.co:

This example is for Wiring version 0024+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Acceleromenter ADXL335 Sparkfun breakout by BARRAGAN
Reads values from an accelerometer with X, Y and Z connected to analog inputs 0, 1 and 2 respectively The values read re printed through the serial to be monitored in the console.

    int x, y, z;

    void setup()
    {
      Serial.begin(9600);           // sets the serial port to 9600
    }

    void loop()
    {
      x = analogRead(0);       // read analog input pin 0
      y = analogRead(1);       // read analog input pin 1
      z = analogRead(2);       // read analog input pin 1
      Serial.print("acceleretations are x, y, z: ");
      Serial.print(x, DEC);    // print the acceleration in the X axis
      Serial.print(" ");       // prints a space between the numbers
      Serial.print(y, DEC);    // print the acceleration in the Y axis
      Serial.print(" ");       // prints a space between the numbers
      Serial.println(z, DEC);  // print the acceleration in the Z axis
      delay(100);              // wait 100ms for next reading
    }