Search wiring.org.co:

This example is for Wiring version 0024+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Advanced Output by Nicholas Zambetti
Demonstrates printing with the Serial library Uses a variety of print calls to output the ASCII character mapping *

    void setup()
    {
      Serial.begin(9600);

      // prints title with ending line break
      Serial.println("ASCII Table ~ Character Map");

      // wait for the long string to be sent
      delay(100);
    }

    int number = 33; // first visible character '!' is #33

    void loop()
    {
      Serial.print(number, BYTE);    // prints value unaltered, first will be '!'

      Serial.print(", dec: ");
      Serial.print(number);          // prints value as string in decimal (base 10)
      // Serial.print(number, DEC);  // this also works

      Serial.print(", hex: ");
      Serial.print(number, HEX);     // prints value as string in hexadecimal (base 16)

      Serial.print(", oct: ");
      Serial.print(number, OCT);     // prints value as string in octal (base 8)

      Serial.print(", bin: ");
      Serial.println(number, BIN);   // prints value as string in binary (base 2)
                                     // also prints ending line break

      // if printed last visible character '~' #126 ...
      if(number == 126) {
        // loop forever
        while(true) {
          continue;
        }
      }

      number++; // to the next character

      delay(100); // allow some time for the Serial data to be sent
    }