Search wiring.org.co:

Reference for Wiring version 0024+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Class | Servo
Name | ### write()
Examples |
    #include "Servo.h"

    Servo myservo;

    void setup() {
      myservo.attach(2)   // attaches a servo connected to pin 2
    }

    void loop() {
      myservo.write(90);  // sets the servo position at 90 degrees
    }
    #include "Servo.h"

    Servo myservo;

    void setup() {
      myservo.attach(3)     // attaches a servo connected to pin 3
    }

    void loop() {
      myservo.write(180);  // sets the servo position at 180 degrees
    }
Description | The write(degrees) method sets the position of the servo to the degrees specified. Servos can be positioned between 0 and 180 degrees. An invalid angle that is valid as pulse in microseconds is treated as microseconds.
Syntax |
    servo.write(degrees)
Parameters |
servo | Any variable of type Servo
degrees | Any integer value between 0 and 180
Returns | None
Usage | Application

Updated on November 01, 2009 08:34:33am PST