Search wiring.org.co:

Reference for Wiring version 0024+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name | ### QSlide
Examples |
    #include "QSlide.h"

    /* create a new QSlide instance
       pin 2: data ready   (drdy)
       pin 3: data in      (sdi)
       pin 4: slave select (ss)
       pin 5: clock        (sclk)
       pin 6: data out     (sdo)
       pin 7: detect       (detect)
       pin 8: proximity    (prox)
    */
    QSlide slider = QSlide(2, 3, 4, 5, 6, 7, 8);

    void setup()
    {
      Serial.begin(9600);      // begin serial communication at 9600bps
    }

    void loop()
    {
      if(slider.isTouching())  // if someone is touching the slider
      {
        int x = slider.read(); // read the slider as an integer
        Serial.print(x);       // print via serial port
      }
    }
Description | The QSlide library allows for manipulating QPROX QSlide sensors.
Syntax |
    QSlide(drdy, sdi, ss, sclk, sdo, detect, prox)
Methods |
isTouching() |
isNear() |
read() |
Parameters |
drdy | The pin connected to the QSlide sensor data ready signal
sdi | The pin connected to the QSlide sensor data in signal
ss | The pin connected to the QSlide sensor slave select signal
sclk | The pin connected to the QSlide sensor clock signal
sdo | The pin connected to the QSlide sensor data out signal
detect | The pin connected to the QSlide sensor detect signal
prox | The pin connected to the QSlide sensor proximity signal
Returns | None
Usage | Application

Updated on November 01, 2009 12:53:53am PDT