Search wiring.org.co:

Index \ Processing \ BasicX \ C The Wiring environment is written in C/C++ and the Processing environment is written in Java so there are many similarities between these two languages. Large distinctions occur with arrays declaration, loops syntax and the printing command. Wiring is used to create programs that run in the Wiring hardware. Processing is used to create programs that run on a PC.

Wiring | Processing
int x = 70; // Initialize x = 30; // Change value | int x = 70; // Initialize x = 30; // Change value
float x = 70.0; x = 30.0; | float x = 70.0; x = 30.0;
int[] a = {5, 10, 11}; // Create an array a[0] = 12; // Reassign | int[] a = {5, 10, 11}; // Create an array a[0] = 12; // Reassign
int a[8]; // Declare a[0] = 1; // Initialize | int[] a = new int[8]; // Declare a[0] = 1; // Initialize
int *a = new int[8]; // Declare a[0] = 1; // Initialize | int[] a = new int[8]; // Declare a[0] = 1; // Initialize

Wiring | Processing
void setup() { // Statements } void loop() { // Statements } | void setup() { // Statements } void draw() { // Statements }
for(int a=45; a<=55; a++) { // Statements } | for(int a=45; a<=55; a++) { // Statements }
if(c==1) { // Statements } | if(c==1) { // Statements }
if(c!=1) { // Statements } | if(c!=1) { // Statements }
if(c < 1) { // Statements } | if(c < 1) { // Statements }
if(c >= 1) { // Statements } | if(c >= 1) { // Statements }
if((c >= 1) && (c < 20)) { // Statements } | if((c >= 1) && (c < 20)) { // Statements }
if(c >= 20) { // Statements 1 } else if (c == 0) { // Statements 2 } else { // Statements 3 } | if(c >= 20) { // Statements 1 } else if (c == 0) { // Statements 2 } else { // Statements 3 }

Wiring | Processing
// Comment | // Comment
void doIt(int x) { // Statements } doIt(x); | void doIt(int x) { // Statements } doIt(x);
int square(int x) { return x*x; } square(X); | int square(int x) { return x*x; } square(X);

Wiring | Processing
Serial.println("hello world"); | println("hello world");
int a = 55; Serial.print(a, DEC); | int a = 55; print(a);
int a = 55; Serial.print("a is "); Serial.print(a, DEC); | int a = 55; print("a is " + a);