| Index

| Reference for Wiring 1.0 (ALPHA) 0020+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### INPUT
Examples |  |
    pinMode(0, INPUT);    // set the pin 0 as an input pin
    pinMode(48, OUTPUT);  // set the pin 48 as an output pin
    portMode(1, OUTPUT);  // set port 1 as an output port
Description |  | Reserved word representing the mode of an I/O pin or and I/O port as an input.
Syntax |  |
    INPUT
Usage |  | Web & Application
Related |  | OUTPUT pinMode() portMode()