| Index

| Reference for Wiring 1.0 (ALPHA) 0021+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### & (bitwise AND)
Examples |  |
    unsigned int a = 60;	// 60 = 0011 1100
    unsigned int b = 13;	// 13 = 0000 1101
    unsigned int c = 0;

    c = a & b;              // 12 = 0000 1100
Description |  | Compares two expressions bit by bit and returns 1 for a position bit if both compared postitions are 1. Returns 0 for that position bit if one or both compared positions are 0. The following list shows all possible combinations: `1 & 0 // Evaluates 0 because the second is 0 0 & 1 // Evaluates 0 because the first is 0 1 & 1 // Evaluates 1 because both are 1 0 & 0 // Evaluates 0 because both are 0`
Syntax |  |
    expression1 & expression2
Parameters |  |
expression1 |  | any valid expression
expression2 |  | any valid expression
Returns |  |
Usage |  | Application
Related |  | &= (bitwise AND and assign) | (bitwise OR) |= (bitwise OR and assign) ^ (bitwise XOR) ˜ (bitwise ones complement) << (bitwise bit shift left) >> (bitwise bit shift right)