| Index

| Reference for Wiring 1.0 (ALPHA) 0021+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### attached()
Examples |  |
    #include <Servo.h>

    Servo myservo;

    void setup() {
      myservo.attach(2)  // attaches a servo connected to pin 2
    }

    void loop() {
      if(myservo.attached()) {
        myservo.write(90);  // position the servo angle at 90 degrees
        myservo.detach();
      }
    }
Description |  | Returns 1 if a servo is attached.
Syntax |  |
    servo.attached()
Parameters |  |
servo |  | Any variable of type Servo
Returns |  | boolean
Usage |  | Application