| Index

| Reference for Wiring 1.0 (ALPHA) 0021+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### degrees()
Examples |  |
    float rad = PI/4;
    float deg = degrees(rad);
    Serial.print(rad);
    Serial.print(" radians is ");
    Serial.print(deg);
    Serial.print(" degrees");
Description |  | Converts a radian measurement to its corresponding value in degrees. Radians and degrees are two ways of measuring the same thing. There are 360 degrees in a circle and 2*PI radians in a circle. For example, 90° = PI/2 = 1.5707964. All trigonometric methods in Wiring require their parameters to be specified in radians.
Syntax |  |
    degrees(angle)
Parameters |  |
angle |  | int or float
Returns |  | float
Usage |  | Web & Application
Related |  | radians()