| Index

| Reference for Wiring 1.0 (ALPHA) 0021+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name |  | ### bitWrite
Examples |  |
    byte x = 33; // sets x to 33 (00100001 in binary)
    bitWrite(x, 2, 1);	// writes a 1 to the second bit bit of x, now x is 00100101 (37 in decimal)
Description |  | The bitWrite command writes 0 or 1 to de desired bit of a byte variable.
Syntax |  |
    bitWrite(byteValue, bitIndex, bitValue)
Parameters |  |
byteValue |  | byte: the byte variable to write the bit to
bitIndex |  | int: the bit to write
bitValue |  | int: the value to write 0 or 1
Returns |  | None
Usage |  | Application
Related |  | bit() bitRead() lowByte() highByte() makeWord()