Search wiring.org.co:

Reference for Wiring version 0024+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name | ### degrees()
Examples |
    float rad = PI/4;
    float deg = degrees(rad);
    Serial.print(rad);
    Serial.print(" radians is ");
    Serial.print(deg);
    Serial.print(" degrees");
Description | Converts a radian measurement to its corresponding value in degrees. Radians and degrees are two ways of measuring the same thing. There are 360 degrees in a circle and 2*PI radians in a circle. For example, 90° = PI/2 = 1.5707964. All trigonometric methods in Wiring require their parameters to be specified in radians.
Syntax |
    degrees(angle)
Parameters |
angle | int or float
Returns | float
Usage | Web & Application
Related | radians()

Updated on January 11, 2010 09:41:50pm PST