Search wiring.org.co:

This example is for Wiring version 0024+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Timer by BARRAGAN
Demonstrates how to create a timer to print a message every 7 seconds

    unsigned long previousTime = 0;

    void setup()
    {
      Serial.begin(9600);
      previousTime = millis();  // mark the initial time
    }

    void loop()
    {
      // if 7 seconds have passed since last mark
      if((millis() - previousTime) >= 7000 ) {
         Serial.println("seven seconds have passed");  //print message
         previousTime = millis();  // mark again
      }
    }