Search wiring.org.co:

Reference for Wiring version 0024+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Class | LiquidCrystal
Name | ### home()
Examples |
    #include "LiquidCrystal.h"

    LiquidCrystal myDisplay = LiquidCrystal(0,1,2,2);
    int a = 0;

    void setup()
    {

    }

    void loop()
    {
      myDisplay.clear();
      myDisplay.home();
      myDisplay.print("Variable a is: ");
      myDisplay.setCursor(16, 0);
      myDisplay.print(a);
      a = a + 1;
      delay(200);
    }
Description | The home() method positions the cursor in the first row and column of the LCD screen.
Syntax |
    display.home()
Parameters |
display | The LiquidCrystal object
Returns | None
Usage | Application

Updated on November 01, 2009 12:41:11am PDT