Search wiring.org.co:

Reference for Wiring version 0024+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name | ### digitalWrite()
Examples |
    int outpin = 0;

    void setup() {
      pinMode(outpin, OUTPUT);
    }

    void loop() {
      digitalWrite(outpin, HIGH);
    }
Description | The digitalWrite() method sets the value of a digital output pin. Possible values are HIGH or LOW.
Syntax |
    digitalWrite(pin,value)
Parameters |
pin | integer value
value | HIGH or LOW
Returns | None
Usage | Application
Related | INPUT OUTPUT HIGH LOW digitalRead() pinMode()

Updated on November 01, 2009 11:25:30pm PST