Search wiring.org.co:

Reference for Wiring version 0024+. If you have a previous version, use the reference included with your software. If you see any errors or have any comments, let us know.

Name | ### LOW
Examples |
    boolean b = true;
    if(b == true) {
      digitalWrite(48, HIGH);  // Turn ON the I/O board LED
    } else {
      digitalWrite(48, LOW);
    }
Description | Reserved word representing the logical value 0 (OFF, 0 volts).
Syntax |
    LOW
Usage | Application
Related | HIGH

Updated on December 03, 2009 07:01:44pm PST