Search wiring.org.co:

This example is for Wiring version 0024+. If you have a previous version, use the examples included with your software. If you see any errors or have comments, please let us know.

Driving a DC Motor by BARRAGAN
Demonstrates the use a DC Motor motor with the L293D Motor Driver chip.

    int motorpin = 0;  // L293D Pin En1 connected to pin PWM 0

    void setup()
    {
      // nothing for setup
    }

    void loop() {
      analogWrite(motorpin, 512);  // turn ON the Motor at medium speed
      delay(100);
    }